{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["办公室搬迁改造方案—电子系"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"办公室搬迁改造方案—电子系","index":0,"n_rows":16,"n_cols":44,"rows_kept":16,"merged":[[0,0,0,43],[1,4,8,4],[1,5,8,5],[1,6,3,11],[1,13,3,13],[1,14,3,14],[1,15,2,15],[1,17,2,17],[1,19,2,19],[1,21,2,21],[1,22,2,22],[1,23,2,23],[1,25,2,25],[1,27,2,27],[1,29,2,29],[1,30,2,30],[1,31,3,33],[1,35,2,35],[1,38,2,38],[1,39,3,39],[1,41,8,41],[1,42,8,42],[1,43,8,43],[3,15,3,22],[3,23,3,30],[4,6,5,14],[4,15,5,20],[4,21,4,22],[4,23,5,28],[4,29,4,30],[4,31,5,36],[4,37,4,38],[4,39,7,40],[5,21,5,22],[5,29,5,30],[5,37,5,38],[6,0,9,3],[6,6,8,11],[6,13,8,14],[6,15,6,22],[6,23,6,30],[6,31,8,33],[6,34,6,38],[7,15,8,15],[7,17,8,17],[7,19,8,19],[7,21,8,22],[7,23,8,23],[7,25,8,25],[7,27,8,27],[7,29,8,30],[7,35,8,35],[7,37,8,38],[9,4,9,43],[10,6,10,40],[10,41,15,41],[10,42,15,42],[10,43,15,43],[11,0,12,1],[11,2,12,3],[11,4,12,5],[11,6,11,40],[12,6,12,40],[13,1,15,1],[13,3,15,3],[13,5,15,5]],"flags":["formulas_cached_only"]}
["1号教学楼2楼办公室搬迁改造方案—电子系"]
["2匹柜式空调（原有）",null,"三孔四位电源插座",null,"楼梯","楼梯",{"$nulls":6},"三孔四位电源插座",null,"3匹柜式空调",null,"三孔四位电源插座",null,"三孔四位电源插座",null,"三孔四位电源插座",null,"3匹柜式空调",null,"三孔四位电源插座",null,"三孔四位电源插座",null,"三孔四位电源插座",null,"3匹柜式空调",{"$nulls":3},"三孔四位电源插座",null,"三孔四位电源插座",null,"3匹柜式空调",null,"三孔三位电源插座","楼梯","楼梯","走廊"]
[null,null,"宽带插座",{"$nulls":9},"电话插座3155650",{"$nulls":3},"四位宽带插座",null,"四位宽带插座",null,"四位宽带插座",{"$nulls":3},"四位宽带插座",null,"四位宽带插座",null,"四位宽带插座",{"$nulls":5},"四位宽带插座",null,"四位宽带插座",{"$nulls":3},"电话插座"]
[{"$nulls":12},"二位宽带插座",{"$nulls":21},"电话插座3156222",{"$nulls":5},"宽带插座"]
["三孔四位电源插座",null,null,"三孔四位电源插座",null,null,"D-1-201系办公室/资料室（预留四台电脑配置）",{"$nulls":8},"D-1-202课程研讨室（预留24台电脑配置）",{"$nulls":5},"三孔四位电源插座",null,"D-1-203课程研讨室/系会议室              （预留24台电脑配置）",{"$nulls":5},"三孔四位电源插座",null,"D-1-204系学生工作办公室/资料室        （预留16台电脑配置）",{"$nulls":5},"三孔四位电源插座",null,"D-1-205系党总支书记办公室"]
["宽带插座",null,null,"宽带插座",{"$nulls":17},"一位宽带插座",{"$nulls":7},"一位宽带插座",{"$nulls":7},"一位宽带插座"]
["接待室/小型会议室（各窗加装防盗网）"]
[{"$nulls":12},"三孔四位电源插座",{"$nulls":3},"三孔四位电源插座",null,"三孔四位电源插座",null,"三孔四位电源插座",{"$nulls":3},"三孔四位电源插座",null,"三孔四位电源插座",null,"三孔四位电源插座",{"$nulls":5},"三孔四位电源插座",null,"三孔四位电源插座"]
[{"$nulls":12},"二位宽带插座",{"$nulls":3},"四位宽带插座",null,"四位宽带插座",null,"四位宽带插座",{"$nulls":3},"四位宽带插座",null,"四位宽带插座",null,"四位宽带插座",{"$nulls":5},"四位宽带插座",null,"四位宽带插座",{"$nulls":3},"1.5匹壁挂空调"]
[{"$nulls":4},"走廊"]
["2匹柜式空调（原有）",null,"1.5匹壁挂空调",null,"1.5匹壁挂空调",null,"注：1.电源插座规格：10A/250V（空调电源插座规格与空调容量匹配）；",{"$nulls":34},"男卫生间","女卫生间","走廊"]
["系主任办公室（窗加装防盗网、建分隔墙）",null,"系副主任办公室（窗加装防盗网、建分隔墙、开独立门）",null,"系副主任办公室（窗加装防盗网、建分隔墙）",null,"    2.插座离地面高300mm安装（壁挂式空调电源插座除外）。"]
[]
["三孔三位电源插座",null,"三孔三位电源插座",null,"三孔三位电源插座"]
["电话插座3156000",null,"电话插座",null,"电话插座"]
["宽带插座",null,"宽带插座",null,"宽带插座"]